DFG reference number: LE 4256/1-1
Project number: 419255448
Project title: A scintillating fibre based beam profile monitor for ion therapy beams
Name(s) of the applicant(s): Dr. Blake Dean Leverington, Ph.D.
Official address(es):  Physikalisches Institut, Im Neuenheimer Feld 226, 69120 Heidelberg

This repository contains the code and documentation for the project. It contains the DAQ software, as well as the electronics design files, and documention. This project was developed by Blake Leverington, Michal Dziewiecki, and Liqing Qin. The project was supported by the Deutsche Forschungsgemeinschaft (DFG), Heidelberg Universitaet, and the Heidelberg Ion-beam Therapy Clinic (HIT).


# HITDAQ

Recomended stable version is in */hit2023v2_RMS* 

The data acquisition software currently compiled with QtCreator on Windows 11, Qt6.5.2, MinGW-11.2.0 64-bit. Needs QtSerialPort.
Also uses QCustomPlot from https://www.qcustomplot.com/release/2.1.1/QCustomPlot-source.tar.gz