This firmware is generted from Simple Socket Server Example. 

M.Dziewiecki created sensor_interface.v in 2019, which controls, collects, and sends ADC data to ethernet.

L.Qin created algo_top_cl_cali_rms.v in 2024, which reconstructs the position and sigma from the ADC data.
