# -------------------------------------------------------------------------- #
#
# Copyright (C) 2018  Intel Corporation. All rights reserved.
# Your use of Intel Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Intel Program License 
# Subscription Agreement, the Intel Quartus Prime License Agreement,
# the Intel FPGA IP License Agreement, or other applicable license
# agreement, including, without limitation, that your use is for
# the sole purpose of programming logic devices manufactured by
# Intel and sold by Intel or its authorized distributors.  Please
# refer to the applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus Prime
# Version 18.0.0 Build 614 04/24/2018 SJ Lite Edition
# Date created = 13:50:14  June 05, 2019
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		hit20v3_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus Prime software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "MAX 10"
set_global_assignment -name DEVICE 10M50DAF484C6GES
set_global_assignment -name TOP_LEVEL_ENTITY m10_rgmii
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 15.0.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "12:52:12  JUNE 15, 2015"
set_global_assignment -name LAST_QUARTUS_VERSION "19.1.0 Lite Edition"
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 2
set_global_assignment -name EDA_SIMULATION_TOOL "ModelSim-Altera (VHDL)"
set_global_assignment -name EDA_OUTPUT_DATA_FORMAT VHDL -section_id eda_simulation
set_location_assignment PIN_M9 -to clk_50_max10
set_location_assignment PIN_D9 -to fpga_resetn
set_location_assignment PIN_T20 -to user_led[0]
set_location_assignment PIN_U22 -to user_led[1]
set_location_assignment PIN_U21 -to user_led[2]
set_location_assignment PIN_AA21 -to user_led[3]
set_location_assignment PIN_AA22 -to user_led[4]
set_location_assignment PIN_L22 -to user_pb[0]
set_location_assignment PIN_M21 -to user_pb[1]
set_location_assignment PIN_M22 -to user_pb[2]
set_location_assignment PIN_N21 -to user_pb[3]
set_location_assignment PIN_H21 -to user_dipsw[0]
set_location_assignment PIN_H22 -to user_dipsw[1]
set_location_assignment PIN_J21 -to user_dipsw[2]
set_location_assignment PIN_J22 -to user_dipsw[3]
set_location_assignment PIN_G19 -to user_dipsw[4]
set_location_assignment PIN_B2 -to qspi_clk
set_location_assignment PIN_C6 -to qspi_io[0]
set_location_assignment PIN_C3 -to qspi_io[1]
set_location_assignment PIN_C5 -to qspi_io[2]
set_location_assignment PIN_B1 -to qspi_io[3]
set_location_assignment PIN_C2 -to qspi_csn
set_location_assignment PIN_Y6 -to enet_mdc
set_location_assignment PIN_Y5 -to enet_mdio
set_location_assignment PIN_T5 -to enet_gtx_clk
set_location_assignment PIN_V8 -to enet_resetn
set_location_assignment PIN_P3 -to enet_rx_clk
set_location_assignment PIN_N9 -to enet_rx_d[0]
set_location_assignment PIN_T1 -to enet_rx_d[1]
set_location_assignment PIN_N1 -to enet_rx_d[2]
set_location_assignment PIN_T3 -to enet_rx_d[3]
set_location_assignment PIN_T2 -to enet_rx_dv
set_location_assignment PIN_E10 -to enet_tx_clk
set_location_assignment PIN_R5 -to enet_tx_d[0]
set_location_assignment PIN_P5 -to enet_tx_d[1]
set_location_assignment PIN_W1 -to enet_tx_d[2]
set_location_assignment PIN_W2 -to enet_tx_d[3]
set_location_assignment PIN_R4 -to enet_tx_en
set_location_assignment PIN_R9 -to enet_led_link100
set_location_assignment PIN_C22 -to mem_a[13]
set_location_assignment PIN_J14 -to mem_a[12]
set_location_assignment PIN_E20 -to mem_a[11]
set_location_assignment PIN_Y20 -to mem_a[10]
set_location_assignment PIN_E22 -to mem_a[9]
set_location_assignment PIN_D22 -to mem_a[8]
set_location_assignment PIN_B20 -to mem_a[7]
set_location_assignment PIN_E21 -to mem_a[6]
set_location_assignment PIN_F19 -to mem_a[5]
set_location_assignment PIN_C20 -to mem_a[4]
set_location_assignment PIN_U20 -to mem_a[3]
set_location_assignment PIN_A21 -to mem_a[2]
set_location_assignment PIN_D19 -to mem_a[1]
set_location_assignment PIN_V20 -to mem_a[0]
set_location_assignment PIN_W22 -to mem_ba[2]
set_location_assignment PIN_N18 -to mem_ba[1]
set_location_assignment PIN_V22 -to mem_ba[0]
set_location_assignment PIN_U19 -to mem_cas_n[0]
set_location_assignment PIN_D18 -to mem_ck[0]
set_location_assignment PIN_E18 -to mem_ck_n[0]
set_location_assignment PIN_W20 -to mem_cke[0]
set_location_assignment PIN_Y22 -to mem_cs_n[0]
set_location_assignment PIN_J15 -to mem_dm[0]
set_location_assignment PIN_K19 -to mem_dq[7]
set_location_assignment PIN_H20 -to mem_dq[6]
set_location_assignment PIN_J20 -to mem_dq[5]
set_location_assignment PIN_H19 -to mem_dq[4]
set_location_assignment PIN_K18 -to mem_dq[3]
set_location_assignment PIN_H18 -to mem_dq[2]
set_location_assignment PIN_K20 -to mem_dq[1]
set_location_assignment PIN_J18 -to mem_dq[0]
set_location_assignment PIN_K14 -to mem_dqs[0]
set_location_assignment PIN_W19 -to mem_odt[0]
set_location_assignment PIN_V18 -to mem_ras_n[0]
set_location_assignment PIN_B22 -to mem_reset_n
set_location_assignment PIN_Y21 -to mem_we_n[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to clk_50_max10
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to fpga_resetn
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_led[0]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_led[1]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_led[2]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_led[3]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_led[4]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_pb[0]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_pb[1]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_pb[2]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_pb[3]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_dipsw[0]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_dipsw[1]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_dipsw[2]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_dipsw[3]
set_instance_assignment -name IO_STANDARD "1.5 V" -to user_dipsw[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_clk
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_io[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_io[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_io[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_io[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to qspi_csn
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_gtx_clk
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_resetn
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_clk
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_d[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_d[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_d[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_d[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_rx_dv
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to enet_tx_clk
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_tx_d[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_tx_d[1]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_tx_d[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_tx_d[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_tx_en
set_instance_assignment -name IO_STANDARD "2.5 V" -to enet_led_link100
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dq[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dq[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "DIFFERENTIAL 1.5-V SSTL CLASS I" -to mem_dqs[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dqs[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "DIFFERENTIAL 1.5-V SSTL CLASS I" -to mem_dqs_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dqs_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "DIFFERENTIAL 1.5-V SSTL CLASS I" -to mem_ck[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_ck[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "DIFFERENTIAL 1.5-V SSTL CLASS I" -to mem_ck_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_ck_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[10] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[11] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[12] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[8] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[9] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_ba[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_ba[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_ba[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_cs_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_we_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_ras_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_cas_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_cke[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_odt[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD 1.5V -to mem_reset_n -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_dm[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name OUTPUT_TERMINATION "SERIES 50 OHM WITHOUT CALIBRATION" -to mem_dm[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name CKN_CK_PAIR ON -from mem_ck_n[0] -to mem_ck[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dq[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DQ_GROUP 9 -from mem_dqs[0] -to mem_dm[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name DM_PIN ON -to mem_dm[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dq[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dm[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dqs[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_dqs_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[10] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[11] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[12] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[3] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[4] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[5] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[6] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[7] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[8] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[9] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ba[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ba[1] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ba[2] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_cs_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_we_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ras_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_cas_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_cke[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_odt[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_reset_n -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ck[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_ck_n[0] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name ENABLE_BENEFICIAL_SKEW_OPTIMIZATION_FOR_NON_GLOBAL_CLOCKS ON -to q_sys_inst|mem_if_ddr3_emif_0 -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name IO_STANDARD "SSTL-15 CLASS I" -to mem_a[13] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_instance_assignment -name PACKAGE_SKEW_COMPENSATION OFF -to mem_a[13] -tag __q_sys_mem_if_ddr3_emif_0_p0
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name UNIPHY_SEQUENCER_DQS_CONFIG_ENABLE ON
set_global_assignment -name OPTIMIZE_MULTI_CORNER_TIMING ON
set_global_assignment -name UNIPHY_TEMP_VER_CODE 2133383589
set_global_assignment -name ECO_REGENERATE_REPORT ON
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "2.5 V"
set_global_assignment -name CYCLONEII_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name SYNTH_TIMING_DRIVEN_SYNTHESIS ON
set_global_assignment -name OPTIMIZE_HOLD_TIMING "ALL PATHS"
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
set_global_assignment -name ENABLE_SIGNALTAP ON
set_global_assignment -name USE_SIGNALTAP_FILE output_files/stp2.stp
set_global_assignment -name PHYSICAL_SYNTHESIS_COMBO_LOGIC ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_RETIMING ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION ON
set_global_assignment -name PHYSICAL_SYNTHESIS_COMBO_LOGIC_FOR_AREA ON
set_global_assignment -name ROUTER_LCELL_INSERTION_AND_LOGIC_DUPLICATION ON
set_global_assignment -name ROUTER_TIMING_OPTIMIZATION_LEVEL MAXIMUM
set_global_assignment -name QII_AUTO_PACKED_REGISTERS NORMAL
set_global_assignment -name MUX_RESTRUCTURE OFF
set_global_assignment -name ROUTER_CLOCKING_TOPOLOGY_ANALYSIS ON
set_global_assignment -name ADV_NETLIST_OPT_SYNTH_WYSIWYG_REMAP ON
set_global_assignment -name SMART_RECOMPILE OFF
set_global_assignment -name TIMING_ANALYZER_MULTICORNER_ANALYSIS ON
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"
set_global_assignment -name INTERNAL_FLASH_UPDATE_MODE "SINGLE IMAGE"
set_global_assignment -name ENABLE_OCT_DONE OFF
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF
set_global_assignment -name CRC_ERROR_OPEN_DRAIN OFF
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -rise
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -fall
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -rise
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -fall
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to mem_a[4]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to mem_a[1]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to mem_a[7]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to mem_a[2]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to user_led[0]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to user_led[2]
set_instance_assignment -name IO_MAXIMUM_TOGGLE_RATE "0 MHz" -to user_pb[1]
set_global_assignment -name EXTERNAL_FLASH_FALLBACK_ADDRESS 00000000
set_location_assignment PIN_E9 -to pmoda[7]
set_location_assignment PIN_A5 -to pmoda[6]
set_location_assignment PIN_A4 -to pmoda[5]
set_location_assignment PIN_D8 -to pmoda[4]
set_location_assignment PIN_B7 -to pmoda[3]
set_location_assignment PIN_A6 -to pmoda[2]
set_location_assignment PIN_C8 -to pmoda[1]
set_location_assignment PIN_C7 -to pmoda[0]
set_location_assignment PIN_B3 -to pmodb[7]
set_location_assignment PIN_B4 -to pmodb[6]
set_location_assignment PIN_A3 -to pmodb[5]
set_location_assignment PIN_A2 -to pmodb[4]
set_location_assignment PIN_C4 -to pmodb[3]
set_location_assignment PIN_B5 -to pmodb[2]
set_location_assignment PIN_D5 -to pmodb[1]
set_location_assignment PIN_E8 -to pmodb[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmoda
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to pmodb
set_location_assignment PIN_Y19 -to debug_rxd
set_location_assignment PIN_W18 -to debug_txd
set_location_assignment PIN_P12 -to adc_cnv[1]
set_instance_assignment -name IO_STANDARD LVDS -to adc_cnv[1]
set_location_assignment PIN_R12 -to "adc_cnv[1](n)"
set_location_assignment PIN_V16 -to adc_cnv[0]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sck[1]
set_instance_assignment -name IO_STANDARD LVDS -to adc_cnv[0]
set_location_assignment PIN_U15 -to "adc_cnv[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to adc_cnv
set_location_assignment PIN_V12 -to adc_sck[1]
set_location_assignment PIN_V11 -to "adc_sck[1](n)"
set_location_assignment PIN_Y14 -to adc_sck[0]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sck[0]
set_location_assignment PIN_Y13 -to "adc_sck[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to adc_sck
set_location_assignment PIN_AB20 -to adc_sdo[4]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo[4]
set_location_assignment PIN_AB19 -to "adc_sdo[4](n)"
set_location_assignment PIN_AB11 -to adc_sdo[3]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo[3]
set_location_assignment PIN_AB10 -to "adc_sdo[3](n)"
set_location_assignment PIN_AB18 -to adc_sdo[2]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo[2]
set_location_assignment PIN_AB17 -to "adc_sdo[2](n)"
set_location_assignment PIN_Y16 -to adc_sdo[1]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo[1]
set_location_assignment PIN_AA15 -to "adc_sdo[1](n)"
set_location_assignment PIN_W13 -to adc_sdo[0]
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo[0]
set_location_assignment PIN_W12 -to "adc_sdo[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to adc_sdo
set_location_assignment PIN_U7 -to link_dir[3]
set_instance_assignment -name IO_STANDARD LVDS -to link_dir[3]
set_location_assignment PIN_U6 -to "link_dir[3](n)"
set_location_assignment PIN_W8 -to link_dir[2]
set_instance_assignment -name IO_STANDARD LVDS -to link_dir[2]
set_location_assignment PIN_W7 -to "link_dir[2](n)"
set_location_assignment PIN_AA7 -to link_dir[1]
set_instance_assignment -name IO_STANDARD LVDS -to link_dir[1]
set_location_assignment PIN_AA6 -to "link_dir[1](n)"
set_location_assignment PIN_W10 -to link_dir[0]
set_instance_assignment -name IO_STANDARD LVDS -to link_dir[0]
set_location_assignment PIN_W9 -to "link_dir[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to link_dir
set_location_assignment PIN_AB8 -to link_rx[3]
set_instance_assignment -name IO_STANDARD LVDS -to link_rx[3]
set_location_assignment PIN_AA8 -to "link_rx[3](n)"
set_location_assignment PIN_AB9 -to link_rx[2]
set_instance_assignment -name IO_STANDARD LVDS -to link_rx[2]
set_location_assignment PIN_AA9 -to "link_rx[2](n)"
set_location_assignment PIN_AB7 -to link_rx[1]
set_instance_assignment -name IO_STANDARD LVDS -to link_rx[1]
set_location_assignment PIN_AB6 -to "link_rx[1](n)"
set_location_assignment PIN_Y4 -to link_rx[0]
set_instance_assignment -name IO_STANDARD LVDS -to link_rx[0]
set_location_assignment PIN_Y3 -to "link_rx[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to link_rx
set_location_assignment PIN_W3 -to link_tx[3]
set_instance_assignment -name IO_STANDARD LVDS -to link_tx[3]
set_location_assignment PIN_W4 -to "link_tx[3](n)"
set_location_assignment PIN_W6 -to link_tx[2]
set_instance_assignment -name IO_STANDARD LVDS -to link_tx[2]
set_location_assignment PIN_W5 -to "link_tx[2](n)"
set_location_assignment PIN_AA10 -to link_tx[1]
set_instance_assignment -name IO_STANDARD LVDS -to link_tx[1]
set_location_assignment PIN_Y10 -to "link_tx[1](n)"
set_location_assignment PIN_P10 -to link_tx[0]
set_instance_assignment -name IO_STANDARD LVDS -to link_tx[0]
set_location_assignment PIN_R10 -to "link_tx[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to link_tx
set_location_assignment PIN_AA12 -to sensor_clk[1]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_clk[1]
set_location_assignment PIN_AA11 -to "sensor_clk[1](n)"
set_location_assignment PIN_W16 -to sensor_clk[0]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_clk[0]
set_location_assignment PIN_V15 -to "sensor_clk[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to sensor_clk
set_location_assignment PIN_Y17 -to sensor_reset[1]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_reset[1]
set_location_assignment PIN_AA17 -to "sensor_reset[1](n)"
set_location_assignment PIN_V17 -to sensor_reset[0]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_reset[0]
set_location_assignment PIN_W17 -to "sensor_reset[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to sensor_reset
set_location_assignment PIN_AB13 -to sensor_trig[4]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig[4]
set_location_assignment PIN_AB12 -to "sensor_trig[4](n)"
set_location_assignment PIN_Y11 -to sensor_trig[3]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig[3]
set_location_assignment PIN_W11 -to "sensor_trig[3](n)"
set_location_assignment PIN_AA16 -to sensor_trig[2]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig[2]
set_location_assignment PIN_AB16 -to "sensor_trig[2](n)"
set_location_assignment PIN_AB15 -to sensor_trig[1]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig[1]
set_location_assignment PIN_AA14 -to "sensor_trig[1](n)"
set_location_assignment PIN_AB5 -to sensor_trig[0]
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig[0]
set_location_assignment PIN_AA5 -to "sensor_trig[0](n)"
set_instance_assignment -name IO_STANDARD LVDS -to sensor_trig
set_location_assignment PIN_AA1 -to sensor_gainn
set_location_assignment PIN_AA2 -to sensor_gainp
set_global_assignment -name NUM_PARALLEL_PROCESSORS ALL
set_global_assignment -name EDA_TEST_BENCH_ENABLE_STATUS TEST_BENCH_MODE -section_id eda_simulation
set_global_assignment -name EDA_NATIVELINK_SIMULATION_TEST_BENCH sensor_algo_tb -section_id eda_simulation
set_global_assignment -name EDA_TEST_BENCH_NAME sensor_algo_tb -section_id eda_simulation
set_global_assignment -name EDA_DESIGN_INSTANCE_NAME NA -section_id sensor_algo_tb
set_global_assignment -name EDA_TEST_BENCH_MODULE_NAME sensor_algo_tb -section_id sensor_algo_tb
set_global_assignment -name EDA_TEST_BENCH_FILE ../dev_room_qlq/algo_dev/testbeanch/sensor_algo_tb.sv -section_id sensor_algo_tb
set_global_assignment -name ALLOW_REGISTER_RETIMING OFF
set_global_assignment -name EXTRACT_VERILOG_STATE_MACHINES ON
set_global_assignment -name OPTIMIZATION_MODE "AGGRESSIVE PERFORMANCE"
set_instance_assignment -name IO_STANDARD "DIFFERENTIAL 1.5-V SSTL" -to ddr3_ram_pll_ref_clk_clk
set_location_assignment PIN_N15 -to "ddr3_ram_pll_ref_clk_clk(n)"
set_location_assignment PIN_N14 -to ddr3_ram_pll_ref_clk_clk
set_global_assignment -name VERILOG_FILE debouncer.v
set_global_assignment -name QIP_FILE software/hit20_v3/mem_init/meminit.qip
set_global_assignment -name SDC_FILE m10_rgmii.out.sdc
set_global_assignment -name QIP_FILE enet_gtx_clk_ddio/enet_gtx_clk_ddio.qip
set_global_assignment -name QIP_FILE clkctrl/synthesis/clkctrl.qip
set_global_assignment -name QIP_FILE q_sys/synthesis/q_sys.qip
set_global_assignment -name VERILOG_FILE m10_rgmii.v
set_global_assignment -name SLD_NODE_CREATOR_ID 110 -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_ENTITY_NAME sld_signaltap -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_clk -to ddr3_ram_pll_ref_clk_clk -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_RAM_BLOCK_TYPE=AUTO" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_NODE_INFO=805334528" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_POWER_UP_TRIGGER=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STORAGE_QUALIFIER_INVERSION_MASK_LENGTH=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ATTRIBUTE_MEM_MODE=OFF" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_FLOW_USE_GENERATED=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_BITS=2" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_FLOW_MGR_ENTITY=sld_reserved_hit20v3_auto_signaltap_0_flow_mgr_c90c" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_BUFFER_FULL_STOP=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_CURRENT_RESOURCE_WIDTH=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INCREMENTAL_ROUTING=1" -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[4] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[7] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[8] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[10] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[12] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[19] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[20] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[23] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_IN_ENABLED=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_PIPELINE=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_RAM_PIPELINE=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_COUNTER_PIPELINE=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ADVANCED_TRIGGER_ENTITY=basic,1," -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL_PIPELINE=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ENABLE_ADVANCED_TRIGGER=0" -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[0] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[1] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[5] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[13] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[14] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[18] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[22] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[26] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[28] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[30] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[0] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_startofpacket" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[1] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|to_udp_endofpacket" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_BITS=2" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STORAGE_QUALIFIER_BITS=141" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK=000000000000000000000" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK_LENGTH=21" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SEGMENT_SIZE=2048" -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[2] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[3] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[15] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[16] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[17] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[24] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[27] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[29] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SAMPLE_DEPTH=2048" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[0] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[1] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[2] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[3] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[4] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[5] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[14]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[6] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[15]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[7] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[8] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[9] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[10] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[11] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[12] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[13] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[14] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[15] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[16] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[17] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[18] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[19] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[20] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[21] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[22] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[23] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[24] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|cali_fac_buffer[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[25] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[26] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[27] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[28] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[29] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[30] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[31] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[32] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[33] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_address_a[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[34] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[35] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[36] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[37] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[38] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[39] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[14]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[40] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[15]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[41] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[16]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[42] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[17]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[43] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[18]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[44] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[19]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[45] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[46] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[20]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[47] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[21]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[48] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[22]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[49] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[23]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[50] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[24]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[51] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[25]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[52] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[26]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[53] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[27]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[54] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[28]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[55] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[29]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[56] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[57] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[30]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[58] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[31]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[59] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[60] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[61] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[62] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[63] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[64] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[65] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_data_a[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[66] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[67] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[68] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[69] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[70] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[71] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[72] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[73] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[74] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|address_a[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[75] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[76] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[77] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[78] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[79] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[80] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[14]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[81] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[15]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[82] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[16]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[83] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[17]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[84] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[18]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[85] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[19]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[86] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[87] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[20]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[88] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[21]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[89] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[22]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[90] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[23]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[91] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[24]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[92] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[25]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[93] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[26]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[94] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[27]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[95] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[28]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[96] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[29]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[97] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[98] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[30]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[99] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[31]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[100] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[101] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[102] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[103] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[104] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[105] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[106] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_ram:data_caled_ram0|data_a[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[107] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_caled_wren_a" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[108] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[109] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[110] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[111] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[112] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[113] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[14]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[114] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[15]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[115] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[116] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[117] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[118] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[119] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[120] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[121] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[122] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[123] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_data[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[124] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_ready" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[125] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_startofpacket" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[126] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|data_in_valid" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[127] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[128] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[129] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[130] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[131] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[132] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[133] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[134] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[135] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|read_cali_address[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[136] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|to_udp_endofpacket" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[137] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|to_udp_ready" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[138] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|to_udp_startofpacket" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[139] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|algo_top_cl_cali_rms:recon|calibration:calibration0|to_udp_valid" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[140] -to "q_sys:q_sys_inst|sensor_algo:sensor_interface|waitrequest" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_DATA_BITS=141" -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[6] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[9] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[11] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[21] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[25] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[31] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_global_assignment -name SLD_FILE db/stp2_auto_stripped.stp
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top